* **Connect Power supply + ignition and connect to positive terminal of DSO.**

Once the process got done (button press)

* Remove ignition and connect only power supply to Positive terminal of DSO.
* Ground to Negative terminal of the DSO.

